<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="101.6" y1="83.82" x2="101.6" y2="0" width="0" layer="20"/>
<wire x1="101.6" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="83.82" width="0" layer="20"/>
<wire x1="0" y1="83.82" x2="101.6" y2="83.82" width="0" layer="20"/>
</plain>
<libraries>
<library name="con-vg">
<description>&lt;b&gt;VG Connectors (DIN 41612/DIN 41617)&lt;/b&gt;&lt;p&gt;
The library contains devices which allow to place the contacts individually or 
in one or several blocks.&lt;p&gt;
This behavior is indicated by the key words &lt;i&gt;single&lt;/i&gt; and &lt;i&gt;block&lt;/i&gt; in
the respective device descriptions.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FAB64S">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
female, 64 pins, type B, rows AB, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="MF_Passives">
<packages>
<package name="R1206">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 1206 Package for Resistors&lt;br/&gt;</description>
</package>
<package name="R0402">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0402 Package for Resistors&lt;br/&gt;</description>
</package>
<package name="CP4MM">
<description>&lt;b&gt;Description:&lt;/b&gt; 4MM Round Package for Electrolytic Capacitors. Based on Panasonic Electrolytic Capacitors.&lt;br&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0603 Package for Capacitors&lt;br/&gt;</description>
</package>
<package name="RA1206">
<description>&lt;b&gt;Description:&lt;/b&gt; Quad Resistor Array Package. Based on Bourns CAY16 series array resistors.&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="MF_Discrete_Semiconductor">
<packages>
<package name="SOD-123">
<description>&lt;b&gt;Description:&lt;/b&gt; Footprint for Diodes in SOD-123 Standard.&lt;br/&gt;</description>
</package>
<package name="SMA">
<description>&lt;b&gt;Description:&lt;/b&gt; Footprint for Diodes in SMA Standard.&lt;br/&gt;</description>
</package>
<package name="SOT-23-3">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard SOT-23-3 footprint.&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="on-nb351x">
<packages>
<package name="SOIC8">
<description>&lt;b&gt;SOIC-8&lt;/b&gt; CASE 751-07&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF&lt;p&gt;
&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt;PLATIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tlc27l2.pdf</description>
</package>
</packages>
</library>
<library name="con-amp">
<description>&lt;b&gt;AMP Connectors&lt;/b&gt;&lt;p&gt;
RJ45 Jack connectors&lt;br&gt;
 Based on the previous libraris:
 &lt;ul&gt;
 &lt;li&gt;amp.lbr
 &lt;li&gt;amp-j.lbr
 &lt;li&gt;amp-mta.lbr
 &lt;li&gt;amp-nlok.lbr
 &lt;li&gt;amp-sim.lbr
 &lt;li&gt;amp-micro-match.lbr
 &lt;/ul&gt;
 Sources :
 &lt;ul&gt;
 &lt;li&gt;Catalog 82066 Revised 11-95 
 &lt;li&gt;Product Guide 296785 Rev. 8-99
 &lt;li&gt;Product Guide CD-ROM 1999
 &lt;li&gt;www.amp.com
 &lt;/ul&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FLOP-4V">
<description>&lt;b&gt;Power connector (Floppy Drive)&lt;/b&gt;&lt;p&gt;
MATE N-LOCK</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE20-2">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
<package name="FE04-2">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
<library name="MF_Connectors">
<packages>
<package name="MF-MICROSD">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for Micro SD Card Slot connector. Based on 4uconnector 15882.&lt;br&gt;</description>
</package>
<package name="PTH_2.54MM_01X02">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for 2.54MM Pitch Header 2 Position. Based on 4UCON 00834.&lt;br&gt;</description>
</package>
<package name="PTH_2.54MM_01X06">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for 2.54MM Pitch Header 6 Position. Based on 4UCON 00834.&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="hpa-idtqs">
<description>IDT QuickSwitches</description>
<packages>
<package name="QVSOP80">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="F15HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="micro-philips">
<description>&lt;b&gt;Philips Microcontroller Devices&lt;/b&gt;&lt;p&gt;
http://www-eu2.semiconductors.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TSSOP16">
<description>&lt;b&gt;TSSOP16: plastic thin shrink small outline package; 16 leads; body width 4.4 mm&lt;/b&gt; SOT403-1&lt;p&gt;
Source: PCA9534_3.pdf</description>
</package>
</packages>
</library>
<library name="con-cuistack">
<description>Audio connectors made by Cui Stack</description>
<packages>
<package name="SJ-3523-SMT">
</package>
</packages>
</library>
<library name="74xx-little-us">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DCK_R-PDSO-G6">
<description>&lt;b&gt;DCK (R-PDSO-G6)&lt;/b&gt; PLASTIC SMALL-OUTLINE PACKAGE&lt;p&gt;
SOT (SC-70) - DCK&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g3157.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X3" library="con-vg" package="FAB64S" value="FAB64S"/>
<element name="R1" library="MF_Passives" package="R1206" value="10k">
<attribute name="VOLTAGE" value=""/>
<attribute name="URL" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="MPN" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="D1" library="MF_Discrete_Semiconductor" package="SOD-123" value="MF-DIO-SOD123-1N4148">
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SOD123-1N4148"/>
<attribute name="POPULATE" value="1"/>
<attribute name="MPN" value="MF-DIO-SOD123-1N4148"/>
<attribute name="HOUSEPART" value="YES"/>
</element>
<element name="U3" library="on-nb351x" package="SOIC8" value="NB3N501"/>
<element name="X6" library="con-amp" package="FLOP-4V" value=""/>
<element name="X1" library="con-lsta" package="FE20-2" value="ESW-120-33-G-D">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="U$1" library="holes" package="3,2" value=""/>
<element name="U$2" library="holes" package="3,2" value=""/>
<element name="U$3" library="holes" package="3,2" value=""/>
<element name="U$4" library="holes" package="3,2" value=""/>
<element name="D3" library="MF_Discrete_Semiconductor" package="SMA" value="SSA33L">
<attribute name="URL" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value="NO"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="D4" library="MF_Discrete_Semiconductor" package="SMA" value="SSA33L">
<attribute name="URL" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value="NO"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="D5" library="MF_Discrete_Semiconductor" package="SMA" value="SSA33L">
<attribute name="URL" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value="NO"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="SD1" library="MF_Connectors" package="MF-MICROSD" value="MF-MICROSD">
<attribute name="URL" value="https://factory.macrofab.com/part/MF-MICROSD"/>
<attribute name="MPN" value="MF-MICROSD"/>
<attribute name="HOUSEPART" value="YES"/>
<attribute name="POPULATE" value="1"/>
</element>
<element name="X2" library="con-lsta" package="FE20-2" value="ESW-120-33-G-D">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
</element>
<element name="QS1" library="hpa-idtqs" package="QVSOP80" value="IDTQS34X2245"/>
<element name="QS2" library="hpa-idtqs" package="QVSOP80" value="IDTQS34X2245"/>
<element name="Q1" library="MF_Discrete_Semiconductor" package="SOT-23-3" value="MF-DSC-SOT233-MMBT3904">
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DSC-SOT233-MMBT3904"/>
<attribute name="MPN" value="MF-DSC-SOT233-MMBT3904"/>
<attribute name="HOUSEPART" value="YES"/>
</element>
<element name="R2" library="MF_Passives" package="R0402" value="10k">
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="J1" library="MF_Connectors" package="PTH_2.54MM_01X02" value="MF-CON-2.54mm-01x02">
<attribute name="LABEL01" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-CON-2.54mm-01x02"/>
<attribute name="LABEL02" value=""/>
<attribute name="MPN" value="MF-CON-2.54mm-01x02"/>
<attribute name="HOUSEPART" value="YES"/>
</element>
<element name="X4" library="MF_Connectors" package="PTH_2.54MM_01X06" value="MF-CON-2.54mm-01x06">
<attribute name="LABEL01" value="GND"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-CON-2.54mm-01x06"/>
<attribute name="LABEL02" value="VCC"/>
<attribute name="LABEL03" value="SDA"/>
<attribute name="LABEL04" value="SCL"/>
<attribute name="LABEL05" value="!INT"/>
<attribute name="MPN" value="MF-CON-2.54mm-01x06"/>
<attribute name="HOUSEPART" value="YES"/>
<attribute name="LABEL06" value="32kHz"/>
</element>
<element name="R3" library="MF_Passives" package="R0402" value="470">
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="R4" library="MF_Passives" package="R0402" value="470">
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="R5" library="MF_Passives" package="R0402" value="2k2">
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="R8" library="MF_Passives" package="R0402" value="2k2">
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="R6" library="MF_Passives" package="R0402" value="470">
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="R7" library="MF_Passives" package="R0402" value="470">
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="C1" library="MF_Passives" package="C0603" value="10 nF">
<attribute name="DIELECTRIC" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="C2" library="MF_Passives" package="C0603" value="10 nF">
<attribute name="DIELECTRIC" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="C3" library="MF_Passives" package="CP4MM" value="4.7 uF">
<attribute name="VOLTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="C4" library="MF_Passives" package="C0603" value="10 nF">
<attribute name="DIELECTRIC" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="C5" library="MF_Passives" package="C0603" value="10 nF">
<attribute name="DIELECTRIC" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="C6" library="MF_Passives" package="CP4MM" value="4.7 uF">
<attribute name="VOLTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="X7" library="adafruit" package="F15HP" value=""/>
<element name="RA1" library="MF_Passives" package="RA1206" value="MF-RES-ARRAY-1K">
<attribute name="VOLTAGE" value="50 V"/>
<attribute name="WATTAGE" value="62 mW"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="MPN" value="MF-RES_ARRAY-1K"/>
<attribute name="HOUSEPART" value="YES"/>
</element>
<element name="RA2" library="MF_Passives" package="RA1206" value="MF-RES-ARRAY-1K">
<attribute name="VOLTAGE" value="50 V"/>
<attribute name="WATTAGE" value="62 mW"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="MPN" value="MF-RES_ARRAY-1K"/>
<attribute name="HOUSEPART" value="YES"/>
</element>
<element name="RA3" library="MF_Passives" package="RA1206" value="MF-RES-ARRAY-1K">
<attribute name="VOLTAGE" value="50 V"/>
<attribute name="WATTAGE" value="62 mW"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="MPN" value="MF-RES_ARRAY-1K"/>
<attribute name="HOUSEPART" value="YES"/>
</element>
<element name="R9" library="MF_Passives" package="R0402" value="100">
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="R10" library="MF_Passives" package="R0402" value="100">
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="MPN" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
<element name="U2" library="micro-philips" package="TSSOP16" value="PCA9557PW">
<attribute name="MPN" value="PCA9557PW,118"/>
<attribute name="MF" value="NXP"/>
</element>
<element name="C7" library="MF_Passives" package="CP4MM" value="10 uF">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
</element>
<element name="X9" library="con-cuistack" package="SJ-3523-SMT" value="SJ-3523-SMT"/>
<element name="X5" library="con-lsta" package="FE04-2" value=""/>
<element name="U4" library="74xx-little-us" package="DCK_R-PDSO-G6" value="74LVC2G04GW"/>
<element name="C8" library="MF_Passives" package="C0603" value="10 nF">
<attribute name="DIELECTRIC" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="HOUSEPART" value=""/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X3" pad="A2"/>
<contactref element="X3" pad="B2"/>
<contactref element="X3" pad="B6"/>
<contactref element="X3" pad="B7"/>
<contactref element="X3" pad="B8"/>
<contactref element="X3" pad="B9"/>
<contactref element="X3" pad="B10"/>
<contactref element="X3" pad="B11"/>
<contactref element="X3" pad="B12"/>
<contactref element="U3" pad="3"/>
<contactref element="SD1" pad="G0"/>
<contactref element="SD1" pad="PIN6"/>
<contactref element="SD1" pad="G1"/>
<contactref element="X3" pad="A4"/>
<contactref element="X2" pad="30"/>
<contactref element="X2" pad="12"/>
<contactref element="QS1" pad="10"/>
<contactref element="QS1" pad="20"/>
<contactref element="QS1" pad="30"/>
<contactref element="QS1" pad="40"/>
<contactref element="X6" pad="2"/>
<contactref element="QS2" pad="10"/>
<contactref element="QS2" pad="20"/>
<contactref element="QS2" pad="30"/>
<contactref element="QS2" pad="40"/>
<contactref element="R1" pad="P$2"/>
<contactref element="X1" pad="12"/>
<contactref element="X1" pad="30"/>
<contactref element="QS1" pad="79"/>
<contactref element="QS1" pad="69"/>
<contactref element="QS1" pad="59"/>
<contactref element="QS1" pad="49"/>
<contactref element="QS2" pad="79"/>
<contactref element="QS2" pad="69"/>
<contactref element="QS2" pad="59"/>
<contactref element="QS2" pad="49"/>
<contactref element="Q1" pad="P$2"/>
<contactref element="X4" pad="P$1"/>
<contactref element="R5" pad="P$1"/>
<contactref element="C1" pad="P$2"/>
<contactref element="C2" pad="P$2"/>
<contactref element="C4" pad="P$2"/>
<contactref element="R8" pad="P$1"/>
<contactref element="C5" pad="P$2"/>
<contactref element="X7" pad="5"/>
<contactref element="X7" pad="8"/>
<contactref element="X7" pad="7"/>
<contactref element="X7" pad="6"/>
<contactref element="X7" pad="10"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="4"/>
<contactref element="C7" pad="P$2"/>
<contactref element="U2" pad="8"/>
<contactref element="X9" pad="1"/>
<contactref element="X5" pad="8"/>
<contactref element="U4" pad="2"/>
<contactref element="C8" pad="P$2"/>
</signal>
<signal name="+5V">
<contactref element="D1" pad="ANODE"/>
<contactref element="X1" pad="11"/>
</signal>
<signal name="+4V1">
<contactref element="R1" pad="P$1"/>
<contactref element="D1" pad="CATHODE"/>
<contactref element="QS1" pad="80"/>
<contactref element="QS1" pad="70"/>
<contactref element="QS1" pad="60"/>
<contactref element="QS1" pad="50"/>
<contactref element="QS2" pad="80"/>
<contactref element="QS2" pad="70"/>
<contactref element="QS2" pad="60"/>
<contactref element="QS2" pad="50"/>
</signal>
<signal name="N$99">
</signal>
<signal name="+3V3">
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="6"/>
<contactref element="X1" pad="29"/>
<contactref element="R2" pad="P$1"/>
<contactref element="SD1" pad="PIN4"/>
<contactref element="X4" pad="P$2"/>
<contactref element="U2" pad="16"/>
<contactref element="C7" pad="P$1"/>
<contactref element="U2" pad="15"/>
<contactref element="X5" pad="1"/>
<contactref element="U4" pad="5"/>
<contactref element="C8" pad="P$1"/>
</signal>
<signal name="-12VABC">
<contactref element="X3" pad="B1"/>
<contactref element="X3" pad="A1"/>
<contactref element="D4" pad="ANODE"/>
</signal>
<signal name="+5VABC">
<contactref element="X3" pad="B31"/>
<contactref element="X3" pad="A31"/>
<contactref element="D5" pad="CATHODE"/>
</signal>
<signal name="+12VABC">
<contactref element="X3" pad="B32"/>
<contactref element="X3" pad="A32"/>
<contactref element="D3" pad="CATHODE"/>
</signal>
<signal name="+5VEXT">
<contactref element="X6" pad="1"/>
<contactref element="D5" pad="ANODE"/>
</signal>
<signal name="+12VEXT">
<contactref element="X6" pad="4"/>
<contactref element="D3" pad="ANODE"/>
</signal>
<signal name="-12VEXT">
<contactref element="X6" pad="3"/>
<contactref element="D4" pad="CATHODE"/>
</signal>
<signal name="N$94">
</signal>
<signal name="XMEMW#/INT#">
<contactref element="X3" pad="A5"/>
<contactref element="QS2" pad="33"/>
</signal>
<signal name="D7">
<contactref element="X3" pad="A6"/>
<contactref element="QS2" pad="27"/>
</signal>
<signal name="D6">
<contactref element="X3" pad="A7"/>
<contactref element="QS2" pad="25"/>
</signal>
<signal name="D5">
<contactref element="X3" pad="A8"/>
<contactref element="QS2" pad="23"/>
</signal>
<signal name="D4">
<contactref element="X3" pad="A9"/>
<contactref element="QS2" pad="38"/>
</signal>
<signal name="D3">
<contactref element="X3" pad="A10"/>
<contactref element="QS2" pad="36"/>
</signal>
<signal name="D2">
<contactref element="X3" pad="A11"/>
<contactref element="QS2" pad="34"/>
</signal>
<signal name="D1">
<contactref element="X3" pad="A12"/>
<contactref element="QS2" pad="32"/>
</signal>
<signal name="D0">
<contactref element="X3" pad="A13"/>
<contactref element="QS2" pad="28"/>
</signal>
<signal name="RESIN#">
<contactref element="X3" pad="A3"/>
<contactref element="QS2" pad="39"/>
</signal>
<signal name="RST#">
<contactref element="X3" pad="A15"/>
<contactref element="QS2" pad="18"/>
</signal>
<signal name="STATUS#">
<contactref element="X3" pad="A16"/>
<contactref element="QS2" pad="14"/>
</signal>
<signal name="INP#">
<contactref element="X3" pad="A17"/>
<contactref element="QS2" pad="8"/>
</signal>
<signal name="C4#">
<contactref element="X3" pad="A18"/>
<contactref element="QS2" pad="5"/>
</signal>
<signal name="C3#">
<contactref element="X3" pad="A19"/>
<contactref element="QS2" pad="9"/>
</signal>
<signal name="C2#">
<contactref element="X3" pad="A20"/>
<contactref element="QS2" pad="13"/>
</signal>
<signal name="C1#">
<contactref element="X3" pad="A21"/>
<contactref element="QS2" pad="15"/>
</signal>
<signal name="OUT#">
<contactref element="X3" pad="A22"/>
<contactref element="QS2" pad="19"/>
</signal>
<signal name="CS#">
<contactref element="X3" pad="A23"/>
<contactref element="QS1" pad="12"/>
</signal>
<signal name="NMI#">
<contactref element="X3" pad="A24"/>
<contactref element="QS1" pad="14"/>
</signal>
<signal name="INP2#">
<contactref element="X3" pad="A25"/>
<contactref element="QS1" pad="16"/>
</signal>
<signal name="XINPSTB#">
<contactref element="X3" pad="A26"/>
<contactref element="QS1" pad="18"/>
</signal>
<signal name="XOUTPSTB#">
<contactref element="X3" pad="A27"/>
<contactref element="QS1" pad="22"/>
</signal>
<signal name="XM#">
<contactref element="X3" pad="A28"/>
<contactref element="QS1" pad="24"/>
</signal>
<signal name="RFSH#">
<contactref element="X3" pad="A29"/>
<contactref element="QS1" pad="26"/>
</signal>
<signal name="RDY">
<contactref element="X3" pad="A30"/>
<contactref element="QS1" pad="28"/>
<contactref element="Q1" pad="P$3"/>
</signal>
<signal name="XMEMWR#">
<contactref element="X3" pad="B3"/>
<contactref element="QS2" pad="37"/>
</signal>
<signal name="XMEMFL#">
<contactref element="X3" pad="B4"/>
<contactref element="QS2" pad="35"/>
</signal>
<signal name="CLK">
<contactref element="X3" pad="B5"/>
<contactref element="QS2" pad="29"/>
<contactref element="QS1" pad="2"/>
</signal>
<signal name="INT#">
<contactref element="X3" pad="B13"/>
<contactref element="QS2" pad="26"/>
</signal>
<signal name="A15">
<contactref element="X3" pad="B14"/>
<contactref element="QS2" pad="24"/>
</signal>
<signal name="A14">
<contactref element="X3" pad="B15"/>
<contactref element="QS2" pad="22"/>
</signal>
<signal name="A13">
<contactref element="X3" pad="B16"/>
<contactref element="QS2" pad="16"/>
</signal>
<signal name="A12">
<contactref element="X3" pad="B17"/>
<contactref element="QS2" pad="12"/>
</signal>
<signal name="A11">
<contactref element="X3" pad="B18"/>
<contactref element="QS2" pad="6"/>
</signal>
<signal name="A10">
<contactref element="X3" pad="B19"/>
<contactref element="QS2" pad="7"/>
</signal>
<signal name="A9">
<contactref element="X3" pad="B20"/>
<contactref element="QS2" pad="4"/>
</signal>
<signal name="A8">
<contactref element="X3" pad="B21"/>
<contactref element="QS2" pad="2"/>
</signal>
<signal name="A7">
<contactref element="X3" pad="B22"/>
<contactref element="QS2" pad="17"/>
</signal>
<signal name="A6">
<contactref element="X3" pad="B23"/>
<contactref element="QS2" pad="3"/>
</signal>
<signal name="MEMRQ#">
<contactref element="X3" pad="B30"/>
<contactref element="QS1" pad="27"/>
</signal>
<signal name="A0">
<contactref element="X3" pad="B29"/>
<contactref element="QS1" pad="25"/>
</signal>
<signal name="A1">
<contactref element="X3" pad="B28"/>
<contactref element="QS1" pad="23"/>
</signal>
<signal name="A2">
<contactref element="X3" pad="B27"/>
<contactref element="QS1" pad="19"/>
</signal>
<signal name="A3">
<contactref element="X3" pad="B26"/>
<contactref element="QS1" pad="17"/>
</signal>
<signal name="A4">
<contactref element="X3" pad="B25"/>
<contactref element="QS1" pad="15"/>
</signal>
<signal name="A5">
<contactref element="X3" pad="B24"/>
<contactref element="QS1" pad="13"/>
</signal>
<signal name="X1IO0">
<contactref element="X1" pad="1"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="X1IO2">
<contactref element="X1" pad="3"/>
<contactref element="QS1" pad="77"/>
</signal>
<signal name="X1IO4">
<contactref element="X1" pad="5"/>
<contactref element="QS1" pad="76"/>
</signal>
<signal name="X1IO6">
<contactref element="X1" pad="7"/>
</signal>
<signal name="X1IO8">
<contactref element="X1" pad="9"/>
<contactref element="QS1" pad="74"/>
</signal>
<signal name="X1IO10">
<contactref element="X1" pad="13"/>
<contactref element="QS1" pad="72"/>
</signal>
<signal name="X1IO12">
<contactref element="X1" pad="15"/>
<contactref element="QS1" pad="68"/>
</signal>
<signal name="X1IO14">
<contactref element="X1" pad="17"/>
<contactref element="QS1" pad="66"/>
</signal>
<signal name="X1IO16">
<contactref element="X1" pad="19"/>
<contactref element="QS1" pad="64"/>
</signal>
<signal name="X1IO18">
<contactref element="X1" pad="21"/>
<contactref element="QS1" pad="62"/>
</signal>
<signal name="X1IO20">
<contactref element="X1" pad="23"/>
<contactref element="QS1" pad="58"/>
</signal>
<signal name="X1IO22">
<contactref element="X1" pad="25"/>
<contactref element="QS1" pad="56"/>
</signal>
<signal name="X1IO24">
<contactref element="X1" pad="27"/>
<contactref element="QS1" pad="54"/>
</signal>
<signal name="X1IO26">
<contactref element="X1" pad="31"/>
<contactref element="QS1" pad="52"/>
</signal>
<signal name="X1IO28">
<contactref element="X1" pad="33"/>
<contactref element="R10" pad="P$1"/>
</signal>
<signal name="X1IO30">
<contactref element="X1" pad="35"/>
<contactref element="RA3" pad="P$3"/>
</signal>
<signal name="X1IO32">
<contactref element="X1" pad="37"/>
<contactref element="RA2" pad="P$3"/>
</signal>
<signal name="X1IO34">
<contactref element="X1" pad="39"/>
<contactref element="RA1" pad="P$3"/>
</signal>
<signal name="X1IO1">
<contactref element="X1" pad="2"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="X1IO3">
<contactref element="X1" pad="4"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="X1IO5">
<contactref element="X1" pad="6"/>
</signal>
<signal name="X1IO7">
<contactref element="X1" pad="8"/>
<contactref element="QS1" pad="75"/>
</signal>
<signal name="X1IO9">
<contactref element="X1" pad="10"/>
<contactref element="QS1" pad="73"/>
</signal>
<signal name="X1IO11">
<contactref element="X1" pad="14"/>
<contactref element="QS1" pad="71"/>
</signal>
<signal name="X1IO13">
<contactref element="X1" pad="16"/>
<contactref element="QS1" pad="67"/>
</signal>
<signal name="X1IO15">
<contactref element="X1" pad="18"/>
<contactref element="QS1" pad="65"/>
</signal>
<signal name="X1IO17">
<contactref element="X1" pad="20"/>
<contactref element="QS1" pad="63"/>
</signal>
<signal name="X1IO19">
<contactref element="X1" pad="22"/>
<contactref element="QS1" pad="61"/>
</signal>
<signal name="X1IO21">
<contactref element="X1" pad="24"/>
<contactref element="QS1" pad="57"/>
</signal>
<signal name="X1IO23">
<contactref element="X1" pad="26"/>
<contactref element="QS1" pad="55"/>
</signal>
<signal name="X1IO25">
<contactref element="X1" pad="28"/>
<contactref element="QS1" pad="53"/>
</signal>
<signal name="X1IO27">
<contactref element="X1" pad="32"/>
<contactref element="QS1" pad="51"/>
</signal>
<signal name="X1IO29">
<contactref element="X1" pad="34"/>
<contactref element="R9" pad="P$1"/>
</signal>
<signal name="X1IO31">
<contactref element="X1" pad="36"/>
<contactref element="RA3" pad="P$1"/>
<contactref element="RA3" pad="P$2"/>
</signal>
<signal name="X1IO33">
<contactref element="X1" pad="38"/>
<contactref element="RA2" pad="P$1"/>
<contactref element="RA2" pad="P$2"/>
</signal>
<signal name="X1IO35">
<contactref element="X1" pad="40"/>
<contactref element="RA1" pad="P$1"/>
<contactref element="RA1" pad="P$2"/>
</signal>
<signal name="X2IO2">
<contactref element="X2" pad="3"/>
</signal>
<signal name="X2IO4">
<contactref element="X2" pad="5"/>
</signal>
<signal name="X2IO6">
<contactref element="X2" pad="7"/>
</signal>
<signal name="X2IO8">
<contactref element="X2" pad="9"/>
</signal>
<signal name="X2IO10">
<contactref element="X2" pad="13"/>
</signal>
<signal name="X2IO12">
<contactref element="X2" pad="15"/>
</signal>
<signal name="X2IO14">
<contactref element="X2" pad="17"/>
</signal>
<signal name="X2IO16">
<contactref element="X2" pad="19"/>
</signal>
<signal name="X2IO18">
<contactref element="X2" pad="21"/>
</signal>
<signal name="X2IO20">
<contactref element="X2" pad="23"/>
</signal>
<signal name="X2IO22">
<contactref element="X2" pad="25"/>
</signal>
<signal name="X2IO24">
<contactref element="X2" pad="27"/>
</signal>
<signal name="X2IO26">
<contactref element="X2" pad="31"/>
</signal>
<signal name="X2IO28">
<contactref element="X2" pad="33"/>
</signal>
<signal name="X2IO30">
<contactref element="X2" pad="35"/>
</signal>
<signal name="X2IO32">
<contactref element="X2" pad="37"/>
</signal>
<signal name="X2IO34">
<contactref element="X2" pad="39"/>
</signal>
<signal name="X2IO35">
<contactref element="X2" pad="40"/>
</signal>
<signal name="X2IO33">
<contactref element="X2" pad="38"/>
</signal>
<signal name="X2IO31">
<contactref element="X2" pad="36"/>
</signal>
<signal name="X2IO29">
<contactref element="X2" pad="34"/>
</signal>
<signal name="X2IO27">
<contactref element="X2" pad="32"/>
</signal>
<signal name="X2IO25">
<contactref element="X2" pad="28"/>
</signal>
<signal name="X2IO23">
<contactref element="X2" pad="26"/>
</signal>
<signal name="X2IO21">
<contactref element="X2" pad="24"/>
</signal>
<signal name="X2IO19">
<contactref element="X2" pad="22"/>
</signal>
<signal name="X2IO17">
<contactref element="X2" pad="20"/>
</signal>
<signal name="X2IO15">
<contactref element="X2" pad="18"/>
</signal>
<signal name="X2IO13">
<contactref element="X2" pad="16"/>
</signal>
<signal name="X2IO11">
<contactref element="X2" pad="14"/>
</signal>
<signal name="X2IO9">
<contactref element="X2" pad="10"/>
</signal>
<signal name="X2IO7">
<contactref element="X2" pad="8"/>
</signal>
<signal name="X2IO5">
<contactref element="X2" pad="6"/>
</signal>
<signal name="X2IO3">
<contactref element="X2" pad="4"/>
</signal>
<signal name="X2IO1">
<contactref element="X2" pad="2"/>
</signal>
<signal name="N$33">
</signal>
<signal name="N$34">
</signal>
<signal name="N$35">
</signal>
<signal name="N$36">
</signal>
<signal name="N$22">
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="FPGARDY#">
<contactref element="R2" pad="P$2"/>
<contactref element="QS1" pad="29"/>
<contactref element="J1" pad="P$1"/>
</signal>
<signal name="X2IO0">
<contactref element="X2" pad="1"/>
</signal>
<signal name="LVCLK">
<contactref element="QS1" pad="78"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="P$2"/>
<contactref element="R4" pad="P$1"/>
<contactref element="C1" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="P$2"/>
<contactref element="C3" pad="P$1"/>
<contactref element="C2" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="P$2"/>
<contactref element="R7" pad="P$1"/>
<contactref element="C4" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="R7" pad="P$2"/>
<contactref element="C6" pad="P$1"/>
<contactref element="C5" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="C3" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="X9" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="C6" pad="P$2"/>
<contactref element="R8" pad="P$2"/>
<contactref element="X9" pad="3"/>
</signal>
<signal name="SD_DI">
<contactref element="SD1" pad="PIN3"/>
</signal>
<signal name="SD_SCLK">
<contactref element="SD1" pad="PIN5"/>
</signal>
<signal name="SD_DO">
<contactref element="SD1" pad="PIN7"/>
</signal>
<signal name="VGA_R">
<contactref element="X7" pad="1"/>
<contactref element="RA1" pad="P$8"/>
<contactref element="RA1" pad="P$7"/>
<contactref element="RA1" pad="P$6"/>
</signal>
<signal name="VGA_G">
<contactref element="X7" pad="2"/>
<contactref element="RA2" pad="P$8"/>
<contactref element="RA2" pad="P$7"/>
<contactref element="RA2" pad="P$6"/>
</signal>
<signal name="VGA_B">
<contactref element="X7" pad="3"/>
<contactref element="RA3" pad="P$8"/>
<contactref element="RA3" pad="P$6"/>
<contactref element="RA3" pad="P$7"/>
</signal>
<signal name="VGA_VS">
<contactref element="X7" pad="14"/>
<contactref element="R10" pad="P$2"/>
</signal>
<signal name="VGA_HS">
<contactref element="X7" pad="13"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="ESP_RESET#">
<contactref element="X5" pad="5"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="ESP_CH_PD">
<contactref element="X5" pad="3"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="N$14">
<contactref element="SD1" pad="PIN2"/>
</signal>
<signal name="N$15">
<contactref element="SD1" pad="PIN10"/>
<contactref element="SD1" pad="PIN9"/>
</signal>
<signal name="ESP_DBG">
<contactref element="X5" pad="6"/>
</signal>
<signal name="ESP_RX">
<contactref element="X5" pad="2"/>
</signal>
<signal name="ESP_IO0">
<contactref element="X5" pad="4"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="ESP_TX">
<contactref element="X5" pad="7"/>
</signal>
<signal name="I2C_SCL">
<contactref element="U2" pad="1"/>
<contactref element="X4" pad="P$4"/>
<contactref element="QS1" pad="4"/>
</signal>
<signal name="I2C_SDA">
<contactref element="U2" pad="2"/>
<contactref element="X4" pad="P$3"/>
<contactref element="QS1" pad="3"/>
</signal>
<signal name="N$10">
</signal>
<signal name="N$2">
<contactref element="R3" pad="P$1"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="P$1"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="P$2"/>
<contactref element="Q1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
